ITEM #: 40 GALLON TILTING KETTLE  
Quantity: One (1)  
Manufacturer: Electrolux  
Model No.: 587041 (PBOT15GDWF)  
Pertinent Data: 40 Gallon  
Utilities Req’d: 120V/1PH; 2.1A; 1” Gas @ 88,634 BTUs; 1/2” CW, 1/2” HW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide digital display of actual cooking/holding temperatures.  
3. Provide digital timer.  
4. Provide unit with a built in food temperature sensor for precise control of cooking process.  
5. Provide unit with a SOFT setting for gentle heat input.  
6. Provide unit with offset tilting axle for convenient pouring height.  
7. Provide unit with left cover plate and water faucet (911821).  
8. KEC shall be responsible for verifying all utilities, dimensions and model number.  
9 Provide four (4) flanged feet (913438) to secure to the floor.  
10. Unit shall be constructed of heavy-gauge stainless steel.  
11. Provide Electrolux Platinum Star Service Program.  
12 Provide 48” quick connect gas hose with a Gas pressure regulator and restraining cable.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.