ITEM #: 40 GALLON TILTING KETTLE  
Quantity: One (1)  
Manufacturer: Groen  
Model No.: DH-40C  
Pertinent Data:   
Utilities Req'd: 120V/1PH; 5.0A; 1/2” Gas @ 100,000 BTUs; 4.5” WC; 1/2” HW, 1/2” CW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer=s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a classic control with Power ONOFF switch with indicator light, temperature control knob with 1 to 10 increments, HEATING indicator light and LOW WATER warning light.  
4. Unit shall be equipped with a 316 stainless steel liner.  
5. Provide a double pantry faucet.  
6. Equip unit with a hinged cover kit.  
7. Unit shall be equipped with a 2” tangent draw-off valve.  
8. Provide kettle interior shall be of type 316 stainless steel, solid one-piece welded construction.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.