ITEM #: 40 QUART TILTING KETTLE  
Quantity: One (1)  
Manufacturer: Groen  
Model No.: TDHC-40C  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 1.0A; 1/2” Gas @ 52,000 BTUs; 5” WC; 1/2” HW, 1/2” CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with a classic control with Power ON-OFF switch with indicator light, temperature control knob with 1 to 10 increments, HEATING indicator light and LOW WATER warning light.  
4. Unit shall be equipped with a 316 stainless steel liner.  
5. Provide a double pantry faucet.  
6. Equip unit with a lift off cover and a cover holder.  
7. Unit shall be equipped with a drain cart and a drain cart plumbing kit.  
8. Provide kettle which shall be of 304 stainless steel, one-piece welded construction. All exposed surfaces shall be stainless steel. All controls shall be contained in a water resistant IPX6rated enclosure.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.