ITEM #: 45 GALLON PRESSURE TILTING SKILLET  
Quantity: One (1)  
Manufacturer: Electrolux  
Model No.: 587028 (PUET17GCWU)  
Pertinent Data: 45 Gallon  
Utilities Req’d: 120V/1PH; 1.7A; 3/4” Gas @ 98,948 BTUs; 7” WC; 1/2” HW, 1/2” CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide digital timer.  
3. Equip unit with a "Pressure function": once the pressure lid is locked, the system automatically regulates itself.  
4. Provide unit with a built-in food temperature sensor for precise control of cooking process.  
5. Provide unit with an electronic microprocessor control system with digital preselection of food cooking temperature, cooking time, and starting time.  
6. Provide unit with a SOFT setting for gentle heat input.  
7. Provide unit with offset tilting axle for convenient pouring height.  
8. KEC shall be responsible for verifying all utilities, dimensions, and model number.  
9. Provide Electrolux Platinum Star Service Program.  
10. Unit shall be constructed of heavy-gauge stainless steel.  
11. Provide left cover plate and a double pantry water faucet (911819).  
12. Equip the unit with a 2” Tangent draw off valve (913571).  
13. Unit shall be supplied with three suspension frames (910191).   
14 Provide four (4) flanged feet (913438) to secure to the floor.  
15 Provide 48” quick connect gas hose with gas pressure regulator and restraining cable.  
16. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.