ITEM # : BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: BBS48  
Pertinent Data: 2 Section, Self-Contained  
Utilities Req’d: 120V/1PH; 5.4A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Back Bar Refrigerator shall be self-contained refrigeration with the condensing unit on the left.  
3. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
4. Provide two (2) solid black vinyl/field laminated doors with full length stainless steel handle, 24". First door hinged left, second door hinged right.  
5. Provide black vinyl coated condensing unit cover.  
6. Provide three (3) flat shelves.  
7. Provide crisp white LED.  
8. Provide four 1-5/8" low-profile casters (63771A), front two with brakes.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.