ITEM # : BACK BAR REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: BBSN72  
Pertinent Data: 3 door, Self-Contained  
Utilities Req’d: 120V/1PH; 6.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Back Bar Refrigerator shall have self-contained refrigeration with the condensing unit on the left.  
3. Provide standard refrigerator (34°F-42°F) factory set to 38°F.  
4. Provide black vinyl coated condensing unit cover.  
5. Unit shall be all stainless steel, unfinished, both sides, and stainless steel top with- no tapping holes.  
6. Provide three sections of solid, black vinyl clad doors.  
7. Door handles to be full-length stainless steel handle, 24".  
8. Provide first and second doors hinged left, and third doo hinged right. Provide all three hinged doors with locks.  
9. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
10. Provide digital thermostat and Crisp White LED interior lighting.  
11. Provide set of six (6) Low Profile Rollers, 1-5/8", front three (3) with brakes.  
12. Unit to have 5 year compressor warranty, 1 year parts and labor warranty.  
13. Provide shop drawings for approval prior to fabrication.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.