ITEM #: BAKERY OVEN  
Quantity: One (1)  
Manufacturer: Gemini  
Model No.: 31  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 47.1A; 120V/1PH; 15.0A; (3) 9.5mm CW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a three-tier deck oven.  
4. Equip the ovens with stone decks.  
5. Each deck will be equipped with a built-in steam generator.  
6. Provide each deck with a digital panel.  
7. Equip the unit with an underbuilt proofer.  
8. Unit shall be equipped with glass doors.  
9. Provide separate controls for top, bottom and front heat.  
10. Provide four (4) heavy-duty, non-marking casters, two (2) with brakes.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.