ITEM #: BASE AND DOME DRYING RACK  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DX1173X50  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 16-gauge 1" diameter 304 stainless steel tubing construction.  
4. Provide 14-gauge stainless steel angle bars and 1@ stainless steel center supports to hold removable cradle inserts.  
5. Provide DX1173XC10 cradles to meet 50 dome capacity.  
6. Provide four (4) 4@ swivel casters, two (2) have locking brakes.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.