ITEM # : BEER DISPENSING TOWER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 4006-4B-Modified  
Pertinent Data: Self-Contained, Eight Faucets  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with faucet locks.  
4. Provide single wide AT@ tower with eight faucets back to back, four on one side four on the other side.  
5. Unit shall have a stainless steel finish.  
6. Equip unit with pure copper coolant lines and cold block maintain chilled beverage temperature.  
7. Unit shall have an insulated dispensing head ensures a perfect temperature right up to the faucet.  
8. Equip unit with Factory-balanced restrictors which control beverage flow and assure solid beer from the faucet with every pour.  
9. Coordinate installation on top of Item \_\_\_\_\_\_, Center Island Bar Top and into Item #\_\_\_\_, Draft Beer Cooler.  
10. Coordinate installation with Item #\_\_\_\_, Drip Trough.  
11. Must meet all applicable governmental, and local laws, rules, regulations, and codes.