ITEM # : BEER DISPENSING TOWER   
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: 4006-6B  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide installation onto and into Item #\_\_\_\_\_, Bar Top and Die.  
4. Provide locking faucet handles.  
5. Coordinate installation with Item #\_\_\_\_\_, Drip Trough.  
6. Unit shall be constructed of 20 gauge stainless steel parts including head, column, drain pan, and perforated inserts.  
7. Equip unit with 16 gauge stainless steel parts including inner column stiffener brackets, 16 gauge galvanized steel parts include: base plate and faucet stiffeners, and 11 gauge stainless steel parts include: inner column base plate.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.