ITEM #: BEER SYSTEM  
Quantity: One (1)  
Manufacturer: Micro Matic  
Model No.: MMPP4301WC  
Pertinent Data: Self-Contained, Water Cooled  
Utilities Req’d: 120V/1PH, 11.6A; 3/8” Chilled Water Supply, 3/8” Chilled Water Return

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Verify line run size, distance and trunk size.  
3. Provide digital thermostat for accurate glycol bath temperature.  
4. Provide a 1/3 HP high-efficiency compressor.  
5. Unit shall insulate cabinet to maintain glycol temperature and minimize condensation.  
6. Coordinate installation onto Item #, Beer System Shelf.  
7. Provide Gas Blender, Secondary Regulator panel, keg couplers and CO2 and Nitrogen regulator.  
8. Provide beer trunk lines and all necessary components.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.