ITEM #: BEVERAGE DRIP TROUGH  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: 1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #23, and #24  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. The unit shall be 94” in length x 5” wide.  
5. Provide a removable stainless steel grate over the drip pan in 13.5” segments to fit into a warewasher.  
6. Equip the removable stainless steel grate with finger holes to allow access to remove it.  
7. Coordinate fabrication and installation with Item #, Beverage Service Counter.  
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.