ITEM #: BOTTLE COOLER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: BC48  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 3.1A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Bottle Cooler shall be self-contained refrigeration.  
3. Provide unit with single access door with lock in lid.  
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with bin dividers.  
6. Unit shall be provided with heavy-duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Coordinate radius curve with the entire bar layout.  
8. Provide the following options and accessories:  
a. Cabinet Finishes  
i. Black Option: Front and ends are black vinyl coated steel (back and bottom galvanized).  
ii. Stainless Steel Option: Front and ends are stainless steel (back and bottom are galvanized).  
iii. All Stainless Steel Option: Front, ends, back and bottom are stainless steel.  
b. Floor Racks.  
c. Bin Dividers.  
d. Interior Light (installed).  
e. Casters.  
f. Speed Rails.  
g. Adjustable Legs.  
h. Bottle Opener and Receiver.  
i. Wine Temperature (specify red or white).  
j. Roller Basket Shelving.  
k. Door Locks.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.