ITEM #: BOTTLE DISPLAY  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TS24LS  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide a five-tier display step unit, with bottle guards on each step.  
4. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.