ITEM #: BUILT-IN BLAST CHILLER  
Quantity: One (1)  
Manufacturer: ThermalRite  
Model No.: GBC837ESK-TS  
Pertinent Data: Double Rack, Remote Compressor, #FS  
Utilities Req’d: 208V/1PH; 20.0A; 1" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide new advanced touch screen controller with USB port on easy-to-use control panel.  
4. Provide unit with Holding cycle which automatically switches over to cooler or freezer mode after each cycle is completed.  
5. Provide one multi point product probe.  
6. Unit shall meet the demands of HACCP Guidelines.  
7. Provide the unit with automatic defrost.  
8. Provide a programmable controller with up to 99 customized options.  
9. Coordinate installation into Item #, Built-In Blast Chiller.  
10. Provide shop drawings for approval prior to installations.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.