ITEM #137: CHARBROILER  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JB-48  
Pertinent Data: Gas  
Utilities Req'd: 3/4" Gas @ 105000 BTU; 5" WC

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide heavy duty cast iron grates with built in grease guides.   
3. Equip with one 15,000 BTU/hr burner every 6" of broiler width controlled by infinite gas valves.   
4. Provide heavy-duty cast iron burner radiants.   
5. Furnish 12-gauge all-welded firebox.   
6. Provide two (2) separate 14-gauge steel drip pans.   
7. Unit to be of 14-gauge, all-welded construction, with stainless steel front, plate shelf, and gas tubing throughout and legs with adjustable feet.   
8. Each burner to be furnished with one stainless steel pilot.   
9. Provide 14-gauge welded drip tray.   
10. Unit to be provided with 3/4" gas regulator.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.