ITEM #: CHARCOAL GRILL AND OVEN  
Quantity: One (1)  
Manufacturer: Josper Basque  
Model No.: CVJ0502HJX25  
Pertinent Data: Solid fuel  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide oven’s firebreak.  
4. Equip the unit with Oven’s Firebreak’s hat.  
5. Unit shall be equipped with storage drawers.  
6. Provide cookware.  
7. Equip the grill portion with Grill’s broiling grill racks, and Grill’s tempering grates.  
8. The Grill portion shall be equipped with two (2) steering wheels to raise and lower the liftable grills.  
9. Equip the unit with fast and agile temperature regulation through the steering wheel of the open grill, which is provided with a hydraulic height regulation system, and through the oven’s vent system.  
10. Provide Oven’s broiling grill rack for the oven section.  
11. Unit shall be equipped with combustion shields.  
12. Provide grease trays.  
13. Equip the unit with Josper tongs, Bristle brush, and Poker.  
14. Unit shall be equipped with an ash drawers.  
15. Provide reutilization of the heat energy produced during the pyrolysis process, both in the oven and in the Basque grill.  
16. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.