ITEM #441: COCKTAIL STATION  
Quantity: One (1)   
Manufacturer: Perlick  
Model No.: TS24IC10  
Pertinent Data: ---  
Utilities Req’d: 1/2" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide TS Series Underbar Ice Bin/Cocktail Unit, modular with cold plate, 24"W x 18-9/16"D, with approximately 50 lbs. ice capacity.  
3. Provide 6" high backsplash with 1" return.  
4. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
5. Provide ABS plastic top ledge, stainless steel top & sides, stainless steel interior, galvanized steel back & bottom.  
6. Provide stainless steel legs with adjustable thermoplastic feet.  
7. Provide ICC24 Ice Chest Covers, 2-piece sliding assembly, 24"W, front & back, and stainless steel.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.