ITEM #: COCKTAIL STATION  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TS36IC10  
Pertinent Data: ---  
Utilities Req’d: 1/2” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” OD stainless steel legs shrouded with stainless steel to conceal the legs.  
3. Provide all type 304 stainless steel construction.  
4. Provide one-piece seamless top and backsplash.  
5. Provide stainless steel interior.  
6. Provide BW6-36 Bottle well.  
7. Coordinate installation of Item #, Bottle Rail and Item # Soda Gun Holder.  
8. Provide unit with cast aluminum cold plate with 2 full length circuits and 8 half-length circuits.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.