ITEM # : COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: AXIOM-TWIN-APS (38700.0013)  
Pertinent Data: ---  
Utilities Req’d: 120/240V/1PH 26.0A; 3/8” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with each 2.5GL PB airpot server (included) has a Safety-Fresh7 brew-through lid with vapor seal and spill protection.  
3. Unit shall include an adjustable bypass which ensures perfect coffee regardless of batch size.  
4. Provide unit with a SplashGard7 funnel which deflects hot liquids away from the hand.  
5. Unit shall have the ability to Brew 5.7L (1-1/2gal) batches.  
6. Must meet all applicable governmental, and local laws, rules, regulations, and codes.