ITEM #: COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: BUNN TF DUAL (34600.0000)  
Pertinent Data: ---  
Utilities Req’d: 120/240V/1PH; 27.5A; 3/8” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have the ability to brew 16.3 to 18.9gal (61.7 to 71.5L) of coffee per hour.   
3. Unit to hold two (2) 1-1/2 gallon ThermoFresh servers.  
4. Equip unit with automatic programming and the ability to store individual recipes.  
5. Unit shall include coffee extraction controlled with pre-infusion and pulse brew, digital temperature control, and large sprayhead; coffee strength controlled with variable by-pass.  
6. Provide SplashGard funnels to deflect hot liquids away from the hand.  
7. Provide ThermoFresh servers that are vacuum insulated to keep coffee hot for hours.  
8. Unit to operate any combination of BrewWISE equipment error-free with wireless brewer-grinder interface through Smart Funnel with SplashGard.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.