ITEM # : COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: DUAL GPR (20900.0011)  
Pertinent Data: ----  
Utilities Req’d: 120/208V/1PH 28.3A; 1/4” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with each 1.5GPR portable server (included) has a Safety-Fresh® brew-through lid with vapor seal and spill protection.  
3. Unit shall include an adjustable bypass which ensures perfect coffee regardless of batch size.  
4. Provide unit with a SplashGard® funnel which deflects hot liquids away from the hand.  
5. Unit shall have the ability to Brew 1-1/2gal (5.7L) batches.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.