ITEM # : COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: ICB Twin (53200.0101)  
Pertinent Data: ---  
Utilities Req’d: 120V/240/1PH, 25A; 3/8” CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with each 1.5GPR portable server (included) has a Safety-Fresh® brew-through lid with vapor seal and spill protection.  
3. Unit shall include an adjustable bypass which ensures perfect coffee regardless of batch size.  
4. Provide unit with a SplashGard® funnel which deflects hot liquids away from the hand.  
5. Unit shall have the ability to Brew 1 1/2gal (5.7L) batches.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.