ITEM # : COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: ICB-DBC TWIN (37600.0002)  
Pertinent Data: ---  
Utilities Req’d: 120/208V/1PH 28.0A; 3/8” CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with BrewMETER® which allows automatic programming of pulse routine.  
3. Unit shall include coffee extraction controlled with pre-infusion and pulse brew, digital temperature control, and large spray head; coffee strength controlled with variable by-pass.  
4. Provide unit with a Funnel which has 28oz (.8kg) ground coffee capacity and paper filter retainers to eliminate fold-over.  
5. Equip the unit with two (2) Airpot 2.5L GL PB (13041.0001).  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.