ITEM #: COFFEE BREWER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: Titan Dual DBC (20900.0008)  
Pertinent Data: ----  
Utilities Req’d: 120/208V/1PH 28.8A; 1/4” CW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Equip unit with BrewMETER® which allows automatic programming of pulse routine.  
3. Unit shall include coffee extraction controlled with pre-infusion and pulse brew, digital temperature control, and large sprayhead; coffee strength controlled with variable by-pass.  
4. Provide unit with a Funnel which has 28oz (.8kg) ground coffee capacity and paper filter retainers to eliminate fold-over.  
5. Unit shall have the ability to Brew up to 34.3 gallons (82.2 liters) of coffee per hour.   
6. Equip the unit with four (4) Titan TF Server Vertical FCT (39400.0001).  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.