ITEM #: COFFEE GRINDER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: 22104.0000  
Pertinent Data: ----  
Utilities Req’d: 120V/1PH 11.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be equipped with a bag switch stops motor when bag is removed and prevents grinding before bag is in place.  
4. Provide fast grinding–one pound in under 30 seconds.  
5. Equip unit with Turbo action draws coffee through grind chamber for greater grinding efficiency.  
6. Unit shall provide a wide range of grinds which can be selected.  
7. Provide a convenient cleaning lever ensures complete clean out of coffee from grind chamber.  
8. Unit shall have a four-year warranty on grinding burrs.  
9. Equip unit with heavy-duty precision burrs for quality, finer grinds.  
10. Provide a single hopper which holds one lb. (0.45 kg) of regular, decaf or specialty coffee beans.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.