ITEM # : COFFEE GRINDER  
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: FPG-2 DBC  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 3.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide portion controlled for the right amount of coffee every time with Multi-batch setting allows user to specify brew size or grind enough coffee into a funnel to brew larger amounts of drip-style coffee  
4. Equip unit with two hoppers each hold 3lb of regular, decaf or specialty coffee beans.  
5. Unit shall be provided with a stainless-steel finish.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.