ITEM # : COFFEE GRINDER   
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: FPG-2 DBC® SST  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 3.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide multi-batch setting allows users to specify a French press brew size or grind enough coffee into a funnel to brew larger amounts of drip-style coffee.  
4. Provide with commercial grinding burrs to provide maximum grinding precision for small amounts of coffee.  
5. Provide two hoppers each hold 3lb (1.36kg) of regular, decaf or specialty coffee beans.  
6. Provide four (4) year warranty on grinding burrs.  
7. Provide professional grind provided by large 3.19” (8.1cm) diameter burrs powered by quiet, low speed, high torque motor.  
8. Provide a stainless steel finish.  
9. Must meet all applicable governmental, and local laws, rules, regulations, and codes.