ITEM # : COFFEE GRINDER   
Quantity: One (1)  
Manufacturer: Bunn  
Model No.: G1 HD BLK  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 11.0A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a bag switch which stops motor when the bag is removed and prevents grinding before the bag is in place.  
4. Provide fast grindingBone pound in under 30 seconds.  
5. Provide turbo action which draws the coffee through the grind chamber for greater grinding efficiency.  
6. Provide a wide range of grinds.  
7. Provide a convenient cleaning lever that ensures complete clean out of coffee from grind chamber.  
8. Provide a four year warranty on grinding burrs.  
9. Coordinate installation onto Item #\_\_\_\_\_.  
10. Must meet all applicable governmental, and local laws, rules, regulations, and codes.