ITEM #: COMBI OVEN  
Quantity: One (1)  
Manufacturer: Blodgett  
Model No.: BLCT-101G  
Pertinent Data: With Stand  
Utilities Req'd: 120V/1PH; 9.0A; (2) 3/4" CW; 2" IW; 3/4" Gas @ 84,000 BTUs; 3.2" -8.0" WC

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 21-1/2" tall stainless steel stand with runners and casters.  
4. Provide 304 stainless steel exterior and interior.  
5. Unit shall have dual pane tempered viewing window with hinged inner glass for easy cleaning.  
6. Equip unit with a door mounted drip tray.  
7. Provide a two-step safety door latch. The first step stops the fan.  
8. Unit shall have an injection steam system - water is injected onto the heating elements, the resulting steam is distributed in the oven chamber by the fan wheel.  
9. Provide the unit with an easy to use touchscreen control, including multiple cooking modes which include hot air, CombiSmart, CombiOptima, retherm, steaming, low-temperature steaming, forced steaming, proofing, and preheating.   
10. Unit shall include manual or automatic cooling.  
11. Provide external core temperature probe.  
12. Provide rack timing which allows for setting individual timers for each rack.  
13. Unit shall be equipped with a reversible 9 speed fan for optimum baking and roasting results.  
14. Equip unit with a USB Port for data and recipe transfer.  
15. Unit shall be provided with HACCP recording and documentation.  
16. Provide automated CombiWash, closed circuit cleaning system features very low water and detergent consumption and no contact with chemicals.  
17. Provide a built-in hand shower.  
18. Provide bright halogen lights.  
19. Provide start-up inspection service by factory authorized service agent.  
20. Provide a backflow preventer.  
21. Coordinate Filtered Water Supply from Item #\_\_\_\_\_\_\_\_\_, Reverse Osmosis System.  
22. Provide 48" flex, quick disconnect gas hose with restraining device and gas pressure regulator.   
23. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.