ITEM #: COMBI OVEN  
Quantity: One (1)  
Manufacturer: Rational  
Model No.: ICP XS E  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 30.0A; 3/4” CW; 1-1/2” IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with iDensityControl is the iCombi Pro’s intelligent climate management. The interaction among intelligent sensors, a high-performance heating system and fresh steam generator, and active dehumidification ensures that the right cooking cabinet climate is always available.   
3. Provide unit with combi steamer mode °F: steam: 86-266, hot air: 86-572, combination: 86-572.   
4. Provide dynamic air circulation in the cooking cabinet thanks to intelligent, reversible, high-performance five-speed fan with intelligent activation and manual programming capabilities.   
5. Provide all type 304 stainless steel construction.   
6. Provide turbo fan cool down function.  
7. High-performance fresh steam generator, pressureless.  
8. Integral, maintenance-free grease extraction system with no additional grease filter.   
9. Provide dynamic air mixing.   
10. Provide unit door with rear ventilated triple-pane glass panel and hinged inner panel.   
11. Provide high-resolution 9 inch TFT color display and capacitative touchscreen with self-explanatory icons for simple, intuitive operation with gestures like swiping and dragging.  
12. Unit shall have acoustic prompts and visual messages when user action is required   
13. Equip with central dial with Push function for intuitive selection and confirmation of entries.  
14. System shall have a user interface and help function which can be set to over 55 languages.  
15. Provide extensive search function including all cooking paths, application examples and settings.  
16. Provide customization and control of user profiles to prevent operator errors.  
17. Equip with interactive notifications regarding cooking paths, requested actions, intelligent functions and warnings thanks to Messenger.   
18. Provide HACCP data output and software update via integral USB port.  
19. Provide unit with Installation kit.  
20. Provide Certified installation by Rational Service Partners.  
21. Provide Preventative Maintenance Kits.  
22. Provide Model R195-CL Water Filtration Single Cartridge System that includes (1) single head with pressure gauge, R95-CL filter & filter installation kit.  
23. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.