ITEM #: CONVEYOR TOASTER  
Quantity: One (1)  
Manufacturer: Hatco  
Model No.: TQ-10  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 8.8A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
3. Provide color guard sensing system for toast uniformity.  
4. Unit shall include a front mounted control panel with a toast selector knob, variable speed control knob, and an aluminum toast collector pan.  
5. Coordinate installation onto Item #, Room Service Chef’s Counter.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.