ITEM # : CORNER DRAIN BOARD  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF-90D-FI  
Pertinent Data: ---  
Utilities Req’d: 1-1/2" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have one-piece seamless top and backsplash featuring 1/4" radius corners for easy cleaning.   
3. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel to conceal the legs.  
4. Unit shall be constructed of a corrugated work surface.   
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.