ITEM #: PLATE DISPENSER  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DXIDPH2E1012 / IDPH2E/1012  
Pertinent Data: Heated  
Utilities Req’d: 120V/1PH; 7.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide mobile heated plate dispenser with enclosed tubular frame.  
4. Equip with two self-elevating dish dispensing tubes.  
5. Provide four 5" casters, two (2) with brakes, and perimeter bumper.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
ITEM #: PLATE SHELF WITH UNDERSHELF LIGHTS (SERVING COUNTER)  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Millwork  
Pertinent Data: See Plans, Drawing #FS   
Utilities Req'd: 120V/1PH, 2.0A

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard Fabrication Drawing #FSX.X, Detail #???.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Coordinate installation with ITEM #, Buffet Counter.  
5. Provide Plate Storage with open shelving on the front of the counter.  
6. Plate storage finish shall be the same as the Solid Surface material chosen for the horizontal surface Verify with the Architect and or Interior De-signer.  
7. Plate storage to have a solid surface material for the bottom and middle shelf.  
8. Provide under shelf lighting for this unit.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.