ITEM #: DISH MACHINE  
Quantity: One (1)  
Manufacturer: Champion  
Model No.: DH6000TVHR  
Pertinent Data: Door Type  
Utilities Req’d: 208V/3PH; 48.0A; 3/4” CW; 1-1/2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide built in 21\*C rise electric booster heater.  
3. Provide single point electrical connection.  
4. Provide rinse sentry to ensure 180⁰ F / 83⁰C final rinse.  
5. Provide autostart when hood is closed.  
6. Provide automatic tank fill.  
7. Provide interchangeable upper and lower spray arms.  
8. Provide bottom mounted digital controls.  
9. Provide ventless heat recovery condensate removal.  
10. Coordinate installation of Item #, Clean Dish Table, and Item #, Soiled Dish Table.  
11. Provide built-in detergent and rinse aid pumps.  
12. Provide Drain Tempering kit.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.