ITEM #: DISPOSER  
Quantity: One (1)  
Manufacturer: In Sink Erator  
Model No.: SS-300-#7-CC-101  
Pertinent Data: Short Body  
Utilities Req'd: 208V/3PH, 3.7A; 1/2" CW, 3" DW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer‘s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide unit with a #7 collar adaptor for installation into Item #, Soiled Dish Table Sink.   
3. Coordinate installation of CC-101 Control Panel.  
4. Provide with solenoid valve, syphon breaker, and flow control valve.   
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.