ITEM #: DOUBLE CONVECTION OVEN  
Quantity: One (1)  
Manufacturer: Blodgett  
Model No.: (2) BDO-100-G-ES  
Pertinent Data: Stacked, Mobile  
Utilities Req’d: (2) 120V/1PH; 8.0A; 3/4” Gas @90,000 BTU’s, WC 3.5”

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide stainless steel front, top and sides.  
4. Provide dual pane thermal glass windows encased in stainless steel door frames.  
5. Provide four (4) 6” heavy-duty, non-marking casters, two (2) with brakes.  
6. Provide tubular black soft touch handle with simultaneous door operation with triple-mounted pressure lock door design with turnbuckle assembly.  
7. Provide double-sided porcelainized baking compartment liner.  
8. Provide gas manifold.  
9. Provide a 48" flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
10. Provide four (4) extra oven racks.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.