ITEM #: DOUBLE CONVECTION OVEN  
Quantity: One (1)  
Manufacturer: Jade Range  
Model No.: JCO-240B  
Pertinent Data: ---  
Utilities Req’d: (2) 120V/1PH; 6.0A; 3/4” Gas @ 110,000 BTU’s, 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit construction shall be full angle-iron frame, with stainless steel front, top, and sides.  
4. Equip unit with one dual pane thermal glass window encased in stainless steel door frame, porcelain door handle with simultaneous door operation and triple-mounted pressure lock door design with turnbuckle assembly.  
5. Provide modular slide out front control panel for easy cleaning.  
6. Equip unit with two stainless steel baking compartment liners, and an aluminized steel combustion chamber.  
7. Unit shall be equipped with dual inlet blower wheel.  
8. Provide electronic spark ignition control system, and removable dual tube burners.  
9. Equip unit with gas pressure regulator as well as a manual gas service cut-off switch located on the front of the control panel.  
10. Unit shall be equipped with solid state thermostat with temperature control range of 200°F (93°C) to 500°F (260°C).  
11. Provide a two-speed fan motor, 1/3 horsepower blower motor with automatic thermal overload protection.  
12. Equip unit with a control area cooling fan, and two 50 watt commercial bake oven lamps.  
13. Provide four (4) 6” heavy-duty, non-marking casters, front two (2) with brakes.  
14. Provide four (4) additional oven racks.  
15. Equip unit with a gas manifold.  
16. Provide 48” flex, quick disconnect gas hose with restraining device and gas pressure regulator.  
17. Provide PosiSet.  
18. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.