ITEM #: DOUBLE SIDED GLASS RACK SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: --

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #46, and #45.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Coordinate installation on Item #, Soiled Dish Table.  
5. Rack shelf is to be 24” wide and placed 10” from edge of table on the ledge side and 10” from the edge of the table on the trough side.  
6. Bottom of shelf is to be 55” AFF maximum.  
7. Shelves shall be 16-gauge stainless steel.  
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.