ITEM #: DOUGH DIVIDER  
Quantity: One (1)  
Manufacturer: Gemini  
Model No.: DIV20E  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH; 4.9A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with 20-part hydraulic divider.  
4. Unit shall have a scaling range of 3.5-32 oz.  
5. Provide unit with a manual operation.  
6. Equip unit with stainless steel blades.  
7. Unit shall have automatic blade retraction.  
8. Unit shall be capable of producing up to 900 pieces per hour.  
9. Provide cast iron head with non-stick coating.  
10. Equip unit with a protection bar handle.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.