ITEM #: DOUGH SHEETER  
Quantity: One (1)  
Manufacturer: Gemini KB Systems  
Model No.: STM 5303  
Pertinent Data: Bench Top  
Utilities Req’d: 208V/3PH; 2.3A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall sheet dough gently and precisely using only a minimum of space.  
4. Equip unit with close to 482mm of working width.  
5. Provide end thickness stop which makes it easy to precisely set desired final thickness.  
6. Unit shall provide consistent final thickness of dough bands.  
7. Unit shall provide uniform product size and weight.  
8. Equip unit with smooth surfaces which make it very easy to clean.  
9. Provide ergonomically shaped roller adjustment lever.  
10. Unit shall have operating elements and controls which are easy to reach.  
11. Unit tables fold up for easy storage and valuable working space.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.