ITEM #: DOUGH SHEETER  
Quantity: One (1)  
Manufacturer: Gemini  
Model No.: SSO685 Automat  
Pertinent Data: ---  
Utilities Req’d: 208V/3PH, 3.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide heavy-duty cord and plug. Coordinate NEMA configuration with the Contractor of Division 16.  
3. Equip unit with 107-3/32” overall length, with a 26” roller length.  
4. Unit shall have a 1/64” to 1-3/4” adjustable roller gap.  
5. Unit shall include a catch pan tray under conveyors.  
6. Provide a 25” width to the conveyor belt.  
7. Provide stainless steel protective guard on each side of rollers.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.