ITEM # : DRAFT BEER COOLER   
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: DDC68  
Pertinent Data: 2 Door, Self-Contained  
Utilities Req’d: 120V/1PH; 2.5A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Back Bar Refrigerator shall be self-contained refrigeration with the condensing unit on the left.  
3. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
4. Provide stainless steel doors and barrel locks hinged left, right.  
5. Provide four (4) 1" casters, front two with brakes.  
6. Coordinate installation of Item #\_\_\_\_, Draft Beer Dispensing Tower, and Item #\_\_\_, Drip Trough.   
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.