ITEM #407: DRAFT BEVERAGE REFRIGERATOR  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: DDS60  
Pertinent Data: Self-Contained  
Utilities Req'd: 120V/1PH; 2.5A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Cooler shall be self contained refrigeration with the condensing unit on the left.  
4. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
5. Provide two (2) solid black vinyl/field laminated doors. First door hinged left, second door hinged right.  
6. Provide stainless steel draft arm.  
7. Provide set of four (4) 1-5/8" low-profile casters (63771A), front two with brakes.  
8. Coordinate installation into Item #\_\_\_\_, Back Bar Counter.  
9. Coordinate installation of Item #\_\_\_\_, Dispensing Tower.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.