ITEM #: DRAINBOARD  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TS12DB  
Pertinent Data: ---  
Utilities Req’d: 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” tubular, stainless steel with 1” adjustable thermoplastic foot and cabinet base.  
3. Provide pitched stainless steel drainboard top, All horizontal and vertical edges 1/4” radius with balled corners.  
4. Provide unit with 6" high backsplash with 1" return.  
5. Provide TS Series 12" W Perforated Drainboard Insert (1040635-12), with 'Stadium' shaped perforations and stainless steel construction.  
6. Provide shop drawings for approval prior to fabrication.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.