ITEM # : DRAINBOARD  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSD18  
Pertinent Data: ---  
Utilities Req’d: 1-1/2" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 1-5/8” tubular, stainless steel with 1” adjustable thermoplastic foot and cabinet base.   
3. Unit shall be constructed of embossed stainless steel drainboard.   
4. Provide shop drawings for approval prior to fabrication.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.