ITEM #: DRAINBOARD  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF18SC  
Pertinent Data: ---  
Utilities Req’d: 1-1/2" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide all stainless steel construction.  
3. Unit shall have 1-5/8" OD stainless steel legs shrouded with stainless steel clip on front panel.  
4. Provide unit with 6" high backsplash with 1" return at top, mechanically fastened and sealed with steel support brackets.  
5. Drainboard to be embossed stainless steel, 21 7/16” deep front to back. All horizontal and vertical edges 1/4” radius with balled corners. Stainless steel drain socket. Drain location is back center.  
6. Provide one (1) adjustable intermediate shelf.  
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.