ITEM #: DRIP TROUGH WITH RINSER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: C18660-GRC  
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” IW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Unit shall be all stainless steel construction.  
4. Provide 4-3/8” diameter heavy-gauge stainless steel glass rack, NSF listed stainless steel rinser.  
5. Equip unit with 1/2” I.D. brass drain tube with 1/2” NPSM thread and mechanical end to accept 1/2” I.D. flexible drain tube.  
6. Coordinate installation into Item #, Bar Top.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.