ITEM # : DRIP TROUGH  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: C18640A-GRC  
Pertinent Data: ---  
Utilities Req'd: 1/2” CW, 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel construction.  
3. Provide unit with glass rinser on center.  
4. Install in-line water regulator set at 15 PSI from the street water supply.  
5. Install in-line one way check valve from the street water supply.  
6. Coordinate installation with Item #, Beer Dispensing Tower.  
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.