ITEM #: DROP-IN HOT FOOD WELL  
Quantity: One (1)  
Manufacturer: Wells Manufacturing  
Model No.: MOD-400TDM/AF  
Pertinent Data: Four Well  
Utilities Req’d: 208V/1PH, 32.0A; 1/4” CW, 1/2” IW (Manifold)  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide factory installed drain manifold, and auto fill.  
3. Provide drain valve extension kit and drain screens.  
4. Hot food well controls shall be installed on counter apron.  
5. Unit shall be pre-wired to controls on apron.  
6. Coordinate installation onto Item #, Service Counter With Sink.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.